				 
      Release Notes for © Benefon (R) BeneWin Exion (TM) 

		        Version 5.0

          (C) Copyright Benefon Oyj, 1996 - 2001
                   All rights reserved.


Other product and company names herein may be the trademarks 
of their respective owners.

This document contains release notes for BeneWin Exion 5.0 program for Windows.  
Information in this document is more current than that in the manuals or 
online Help.

There is some addiotional manuals in <CD ROM DRIVE LETTER>\Manuals directory

========
Contents
========

 1      Software Installation Information
 2      Trouble shooting




=========================================
Part 1: Software Installation Information
=========================================

To install BeneWin Exion 5.0 program, use the Program Manager or File Manager 
to start SETUP.EXE as you would any other Windows-based application.  
For example installing from drive CD ROM:

- From the Program Manager File menu, choose Run.
- In the Run dialog box, type <CD ROM DRIVE LETTER>:\SETUP and choose OK.

  Or

- From the File Manager, double-click the SETUP.EXE file icon 
  on CD ROM drive.


Files installed:

APPLICATION DIRECTORY:
 bwexion.exe	Benewin Exion main program.
 bwexion.hlp	windows help file for Benewin Exion application.
 readme.txt	this information file in ascii format
 _isreg32.dll	Information for uninstalling BeneWin Exion 5.0
 deisl1.isu	Information for uninstalling BeneWin Exion 5.0
 _deisreg.isr	Information for uninstalling BeneWin Exion 5.0


Files updated if newer:

WINDOWS DIRECTORY:
 COMCTL32.OCX
 OLEPRO32.DLL
 OLEAUT32.DLL
 MFC42.DLL
 MSVCRT.DLL
 COMCT232.OCX
 TABCTL32.OCX
 MSCAL.OCX


Icons created:
 Benewin Exion		Start the Benewin Exion application by choosing this icon.
 Benewin Exion help	This is the Benewin windows help file. You can explore 
			help file without starting benewin by choosing this icon.
 Readme			This ascii file for windows notepad or any other ascii editor.

 Exion			Desktop icon for Benewin Exion application.






=========================================
Part 2: Trouble shooting
=========================================

If you have troubles to get connected to your cellular phone with 
Benewin program. Please check out following things:

- Do you use same communication port where you have connected Benewin Exion data cable?

- Power off and power on again the cellular phone and try again. while 
  the mobile phone is powered off remove and replace the battery also.

- If you are using the laptop or portable computer set off 
  the power saving option. 

- Check the comm port settings from the window's controll panel. 
  Change flow controll to NONE. Databits to EIGHT. Stopbits to ONE.

- Is the comm port operational at all? check the IRQs (consult the windows manuals). 
  Other devices like modems block the communication if they use the same IRQ.

- Reboot your computer and cellular phone and try again.

- Check the connector from your computer communication port. 

- Check the Benewin Exion data cable's connectors. 

- Change the Benewin Exion data cable.

